# architecture
BR2_arm=y
BR2_cortex_a8=y
BR2_ARM_EABIHF=y

# system
BR2_TARGET_GENERIC_HOSTNAME="beaglebone"
BR2_ROOTFS_DEVICE_CREATION_DYNAMIC_DEVTMPFS=y
BR2_TARGET_GENERIC_GETTY_PORT="ttyO0"
# BR2_TARGET_GENERIC_REMOUNT_ROOTFS_RW is not set
BR2_ROOTFS_POST_IMAGE_SCRIPT="board/beaglebone/post-image.sh"

# filesystem
BR2_PACKAGE_AM33X_CM3=y
BR2_TARGET_ROOTFS_EXT2=y
# BR2_TARGET_ROOTFS_TAR is not set

# lock down headers to avoid breaking with new defaults
BR2_KERNEL_HEADERS_VERSION=y
BR2_DEFAULT_KERNEL_VERSION="3.12.10"
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_3_12=y

# bootloader
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BOARDNAME="am335x_evm"
BR2_TARGET_UBOOT_CUSTOM_VERSION=y
BR2_TARGET_UBOOT_CUSTOM_VERSION_VALUE="2013.10"
BR2_TARGET_UBOOT_FORMAT_IMG=y
BR2_TARGET_UBOOT_SPL=y
BR2_TARGET_UBOOT_SPL_NAME="MLO"

# kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_GIT=y
BR2_LINUX_KERNEL_CUSTOM_REPO_URL="git://git.ti.com/ti-linux-kernel/ti-linux-kernel.git"
BR2_LINUX_KERNEL_CUSTOM_REPO_VERSION="7f280334068b7c875ade51f8f3921ab311f0c824"
BR2_LINUX_KERNEL_PATCH="board/beaglebone/patches/linux/"
BR2_LINUX_KERNEL_USE_CUSTOM_CONFIG=y
BR2_LINUX_KERNEL_CUSTOM_CONFIG_FILE="board/beaglebone/linux-3.12.config"
BR2_LINUX_KERNEL_ZIMAGE=y
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="am335x-bone am335x-boneblack"
